GSIC - Global Service Information Center

# FUEL LID LOCK CONTROL > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE FRONT SEAT ASSEMBLY (for RHD)

Separate seat type (Click here)
Bench seat type (Click here)

3. REMOVE REAR SEAT ASSEMBLY (for Double Cab)

Remove the seat (Click here).

4. REMOVE REAR SEAT CUSHION ASSEMBLY LH (for Extra Cab)

1. Pull the seat cushion lock hook's release lever in the direction of the arrow, and then disconnect the hook on the front of the seat cushion.

1. Detach the seat cushion's 2 rear hooks from the vehicle body.

1. Remove the seat cushion.

5. REMOVE REAR SEAT CUSHION ASSEMBLY RH (for Extra Cab)

HINT:

  Use the same procedures described for the LH side.

6. REMOVE BACK PANEL GARNISH LOWER (for Extra Cab)

1. Using a screwdriver, detach the 6 claws.

   HINT:
     Tape the screwdriver tip before use.

1. Using a clip remover, detach the 5 clips and remove the garnish.

7. REMOVE CONSOLE BOX ASSEMBLY (for RHD)

1. Remove the 4 screws <F> and 2 bolts <E>.

1. Using a clip remover, remove the 2 clips and console box.

8. REMOVE FRONT DOOR SCUFF PLATE LH

Double cab (Click here)
Single cab and extra cab (Click here)

9. REMOVE FRONT DOOR SCUFF PLATE RH (for RHD)

Double cab (Click here)
Single cab and extra cab (Click here)

10. REMOVE COWL SIDE TRIM BOARD LH (for LHD)

1. Remove the cap nut.

1. Using a clip remover, detach the 2 clips and remove the trim board.

11. REMOVE COWL SIDE TRIM BOARD RH (for RHD)

HINT:

  Use the same procedures described for the LH side.

12. REMOVE REAR DOOR SCUFF PLATE LH (for Double Cab)

1. Using a screwdriver, detach the 7 claws.

   HINT:
     Tape the screwdriver tip before use.

1. Using a clip remover, detach the 2 clips and remove the scuff plate.

13. REMOVE FRONT SEAT OUTER BELT ASSEMBLY LH

1. Single cab:
   Remove the outer belt shoulder anchor.

   1. Using a screwdriver, detach the 2 claws and open the seat belt anchor cover.

      HINT:
        Tape the screwdriver tip before use.

   2. Remove the bolt and shoulder anchor.

1. Double cab:
   Remove the outer belt shoulder anchor.

   1. Using a screwdriver, disengage the 4 claws and remove the seat belt anchor cover cap.

      HINT:
        Tape the screwdriver tip before use.

   2. Remove the bolt and shoulder anchor.

1. w/o Pretensioner:
   Remove the bolt and seat belt.

1. w/ Pretensioner:

   1. Disconnect the pretensioner connector as shown in the illustration.

   2. Remove the bolt and seat belt.

14. REMOVE REAR NO. 1 SEAT BELT ASSEMBLY OUTER LH (for Extra Cab)

1. Remove the bolt and floor anchor.

1. Using a screwdriver, detach the 2 claws and open the seat belt anchor cover.

   HINT:
     Tape the screwdriver tip before use.

1. Remove the bolt.

1. Remove the bolt and seat belt.

15. REMOVE CENTER PILLAR GARNISH LOWER LH (for Double Cab)

1. Using a screwdriver, detach the 2 claws.

   HINT:
     Tape the screwdriver tip before use.

1. Using a clip remover, detach the 2 clips and remove the garnish.

16. REMOVE QUARTER TRIM PANEL LOWER LH

Double cab (Click here)
Single cab (Click here)

17. REMOVE QUARTER INSIDE TRIM BOARD LH (for Extra Cab)

1. Using a clip remover, detach the 7 clips.

1. Using a screwdriver, detach the 6 claws and remove the trim board.

   HINT:
     Tape the screwdriver tip before use.

1. Detach the claws and remove the trim pocket from the trim board.

18. REMOVE FLOOR CARPET ASSEMBLY FRONT (for RHD)

1. Partially remove the floor carpet.

   HINT:
     It is not necessary to fully remove the floor carpet. Partially remove it so that the lock control cable can be removed in a later step.

19. REMOVE REAR NO. 1 WHEEL OPENING EXTENSION LH (w/ Rear wheel opening extension)

1. Remove the 7 screws.

1. Detach the 11 clips and remove the extension.

20. REMOVE REAR WHEEL HOUSE LINER LH

1. Partially remove the liner.

   HINT:
     It is not necessary to fully remove the liner. Partially remove it so that the lock control cable can be removed in a later step.

21. REMOVE FUEL LID LOCK CONTROL CABLE SUB-ASSEMBLY

1. Remove the open lever.

1. Remove the grommet from the vehicle body.

1. Remove the cable from the clamps as shown in the illustration.

1. Turn the lock retainer counterclockwise and remove the cable from the retainer.

22. REMOVE FUEL FILLER OPENING LID LOCK RETAINER

1. Turn the lock retainer clockwise and remove the lock retainer as shown in the illustration.