GSIC - Global Service Information Center

# FLOOR SHIFT ASSEMBLY > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE PARKING BRAKE HOLE COVER SUB-ASSEMBLY

1. Remove the parking brake hole cover sub-assembly (Click here).

3. REMOVE UPPER CONSOLE PANEL SUB-ASSEMBLY

1. Remove the upper console panel sub-assembly (Click here).

4. REMOVE CONSOLE BOX ASSEMBLY

1. Remove the console box assembly (Click here).

5. REMOVE FLOOR SHIFT ASSEMBLY

1. Disconnect the 2 connectors and clamp.

1. Move the shift lever to L.

1. Disconnect the transmission control cable.

1. Remove the 4 bolts.

1. Remove the floor shift.