GSIC - Global Service Information Center

# STOP LIGHT SWITCH > INSTALLATION

## for Preparation Click here

1. INSTALL STOP LIGHT SWITCH ASSEMBLY

1. Install the adjuster to the support.

1. Insert the switch into the adjuster until it slightly touches the pedal.

   NOTICE:
     Do not depress the pedal.

2. ADJUST STOP LIGHT SWITCH ASSEMBLY

3. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

4. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.