GSIC - Global Service Information Center

### CLUTCH UNIT > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE NO. 1 ENGINE COVER SUB-ASSEMBLY (4WD)

3. REMOVE NO. 2 ENGINE COVER SUB-ASSEMBLY (4WD)

4. REMOVE FRONT PROPELLER SHAFT ASSEMBLY (4WD)

5. REMOVE REAR PROPELLER SHAFT ASSEMBLY

6. REMOVE MANUAL TRANSMISSION UNIT ASSEMBLY

7. REMOVE CLUTCH RELEASE BEARING ASSEMBLY

8. REMOVE CLUTCH RELEASE FORK BOOT

9. REMOVE CLUTCH RELEASE FORK SUB-ASSEMBLY

10. REMOVE RELEASE BEARING HUB CLIP

11. REMOVE RELEASE FORK SUPPORT

12. REMOVE CLUTCH COVER ASSEMBLY

13. REMOVE CLUTCH DISC ASSEMBLY

14. INSPECT INPUT SHAFT FRONT BEARING

15. REMOVE INPUT SHAFT FRONT BEARING

16. INSPECT CLUTCH DISC ASSEMBLY

17. INSPECT CLUTCH COVER ASSEMBLY

18. INSPECT FLYWHEEL SUB-ASSEMBLY

19. INSPECT CLUTCH RELEASE BEARING ASSEMBLY