GSIC - Global Service Information Center

# TRANSFER INDICATOR SWITCH > ON-VEHICLE INSPECTION

## for Preparation Click here

1. INSPECT TRANSFER INDICATOR SWITCH (4WD POSITION)

1. Measure the resistance of the switch.

   Standard resistance:

     Tester Connection | Switch Condition | Specified Condition
     1 - 2 | Pushed | Below 1 Ω
     1 - 2 | Not pushed | 10 kΩ or higher

   If the result is not as specified, replace the switch.

2. INSPECT TRANSFER INDICATOR SWITCH (L4 POSITION SWITCH)

1. Measure the resistance of the switch.

   Standard resistance:

     Tester Connection | Switch Condition | Specified Condition
     1 - 2 | Pushed | Below 1 Ω
     1 - 2 | Not pushed | 10 kΩ or higher

   If the result is not as specified, replace the switch.

3. INSPECT TRANSFER INDICATOR SWITCH (NEUTRAL POSITION)

1. Measure the resistance of the switch.

   Standard resistance:

     Tester Connection | Switch Condition | Specified Condition
     1 - 2 | Pushed | Below 1 Ω
     1 - 2 | Not pushed | 10 kΩ or higher

   If the result is not as specified, replace the switch.