GSIC - Global Service Information Center

# 1GR-FE ENGINE CONTROL SYSTEM > TORQUE SPECIFICATIONS

Part Tightened | N*m | kgf*cm | ft.*lbf
Throttle body assembly x Intake manifold | 11 | 112 | 9
Air cleaner assembly x Cylinder head cover sub-assembly | 8.0 | 82 | 71 in.*lbf
Air cleaner assembly x Intake air surge tank | 8.0 | 82 | 71 in.*lbf
V-bank cover x Air cleaner assembly | 7.5 | 76 | 66 in.*lbf
V-bank cover x Intake air surge tank | 7.5 | 76 | 66 in.*lbf
Knock sensor x Cylinder block sub-assembly | 20 | 204 | 15
Water outlet pipe No. 1 x Cylinder block sub-assembly | 10 | 102 | 7
Accelerator pedal rod assembly x Body | 7.5 | 76 | 66 in.*lbf
ECM x Instrument panel reinforcement | 12.5 | 127 | 9
ECM x Blower assembly | 12.5 | 127 | 9
ECM x ECM bracket | 3.0 | 31 | 27 in.*lbf
4WD control ECU x ECM bracket | 12.5 | 127 | 9
Camshaft timing oil control valve x Cylinder head | 9.0 | 92 | 80 in.*lbf
Crankshaft position sensor x Cylinder block | 9.0 | 92 | 80 in.*lbf
Engine coolant temperature sensor x Water by-pass joint rear | 20 | 204 | 15