GSIC - Global Service Information Center

### WATER PUMP > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE NO. 1 ENGINE UNDER COVER

3. DRAIN ENGINE COOLANT

4. DISCONNECT RADIATOR HOSE INLET

5. DISCONNECT RADIATOR HOSE OUTLET

6. REMOVE FAN SHROUD

7. REMOVE GENERATOR ASSEMBLY

8. REMOVE OIL LEVEL GAUGE GUIDE

9. REMOVE NO. 1 IDLER PULLEY SUB-ASSEMBLY

10. REMOVE V-RIBBED BELT TENSIONER ASSEMBLY

11. REMOVE WATER PUMP ASSEMBLY