GSIC - Global Service Information Center

# 1GR-FE ENGINE MECHANICAL > TORQUE SPECIFICATIONS

Part Tightened | N*m | kgf*cm | ft.*lbf
No. 3 camshaft camshaft bearing cap x Cylinder head :10 mm head bolt | 9.0 | 92 | 80
No. 3 camshaft camshaft bearing cap x Cylinder head :12 mm head bolt (A) | 24 | 245 | 18
No. 3 chain tensioner x Cylinder head | 19 | 194 | 14
No. 4 camshaft bearing cap x Cylinder head :10 mm head bolt | 9.0 | 92 | 80
No. 4 camshaft camshaft bearing cap x Cylinder head :12 mm head bolt (A) | 24 | 245 | 18
No. 4 camshaft x Camshaft timing gear | 100 | 1,020 | 74
No. 1 camshaft x Camshaft timing gear | 100 | 1,020 | 74
No. 3 camshaft x Camshaft timing gear | 100 | 1,020 | 74
No. 1 camshaft x Camshaft timing gear | 100 | 1,020 | 74
No. 2 chain tensioner x Cylinder head | 19 | 194 | 14
No. 2 camshaft bearing cap x Cylinder head :10 mm head bolt | 9.0 | 92 | 80 in.*lbf
No. 2 camshaft bearing cap x Cylinder head :12 mm head bolt (A) | 24 | 245 | 18
No. 2 camshaft x Camshaft timing gear | 100 | 1.020 | 74
Chain tensioner x Cylinder block | 10 | 102 | 7
Timing chain cover plate x Timing chain cover | 9.0 | 92 | 80 in.*lbf
Cylinder head cover LH x Cylinder head : for bolt A | 10 | 102 | 7
Cylinder head cover LH x Cylinder head : for bolt B | 9.0 | 92 | 80 in.*lbf
Cylinder head cover LH x Cylinder head : for nut | 9.0 | 92 | 80 in.*lbf
Cylinder head cover RH x Cylinder head : for bolt A | 10 | 102 | 7
Cylinder head cover RH x Cylinder head : for bolt B | 9.0 | 92 | 80 in.*lbf
Cylinder head cover RH x Cylinder head : for nut | 9.0 | 92 | 80 in.*lbf
Ignition coil x Cylinder head cover | 10 | 102 | 7
V-bank cover x V-bank cover bracket | 7.5 | 76 | 66 in.*lbf
Oil filler cap housing x Cylinder head | 9.0 | 92 | 80 in.*lbf
Water by-pass joint x Cylinder head | 9.0 | 92 | 80 in.*lbf
Camshaft timing oil control valve x Cylinder head | 9.0 | 92 | 80 in.*lbf
Intake manifold x Cylinder head | 26 | 265 | 19
V-ribbed belt tensioner x Cylinder block | 36 | 367 | 27
No. 1 idler pulley x Timing chain cover | 54 | 551 | 40
No. 2 idler pulley x Timing chain cover | 39 | 398 | 29
Engine mounting bracket LH x Cylinder block | 43 | 438 | 32
Engine mounting bracket RH x Cylinder blcok | 43 | 438 | 32
Engine mounting bracket x Body | 38 | 387 | 28
Flywheel x Crankshaft | 83 | 846 | 61
Drive plate and ring gear x Crankshaft | 83 | 846 | 61
Exhaust manifold LH x Cylinder head | 30 | 306 | 22
Exhaust manifold RH x Cylinder head | 30 | 306 | 22
Ground cable x Cylinder block | 13 | 133 | 10
Engine wire x Engine room junction block | 13 | 133 | 10
Ground wire x Cylinder block | 31 | 316 | 23
Ground wire x Body | 13 | 133 | 18
A/F sensor bracket x Body | 13 | 133 | 18
Intake air surge tank x Intake manifold | 28 | 286 | 21
Surge tank stay x Intake air surge tank | 21 | 214 | 15
Surge tank stay x Cylinder head | 21 | 214 | 15
Surge tank stay x Oil baffle plate | 9.0 | 92 | 80 in.*lbf
Throttle body bracket x Cylinder head cover | 21 | 214 | 15
Throttle body bracket x Intake air surge tank | 21 | 214 | 15
Vane pump x Timing chain cover | 43 | 438 | 32
Hood x Hood hinge | 11.5 | 117 | 8.5
Crankshaft bearing cap x Cylinder block | 1st: 61 2nd: Turn 90° | 1st: 622 2nd: Turn 90° | 1st: 45 2nd: Turn 90°
Crankshaft main bearing cap bolt x Cylinder block | 35 | 357 | 26
Stud bolt x Cylinder block : for A | 11 | 112 | 8.1
Stud bolt x Cylinder block : for B | 4.5 | 46 | 40 in.*lbf
Stud bolt x Cylinder block : for C | 4.0 | 41 | 35 in.*lbf
Oil nozzle x Cylinder block | 9.0 | 92 | 80 in.*lbf
Connecting rod cap x Connecting rod | 1st: 25 2nd: Turn 90° | 1st: 250 2nd: Turn 90° | 1st: 18 2nd: Turn 90°
Stud bolt x Cylinder head : for A | 4.0 | 41 | 35 in.*lbf
Stud bolt x Cylinder head : for B | 9.0 | 92 | 80 in.*lbf
Union x Cylinder head | 15 | 150 | 11
Head straight screw plug x Cylinder head | 80 | 816 | 59
Engine rear oil seal retainer x Cylinder block | 9.0 | 92 | 80
Knock sensor x Cylinder block | 20 | 204 | 15
No. 1 water outlet pipe x Cylinder block | 9.0 | 92 | 80 in.*lbf
Cylinder head RH x Cylinder block | 1st: 36 2nd: Turn 180° | 1st: 367 2nd: Turn 180° | 1st: 27 2nd: Turn 180°
Cylinder head LH x Cylinder block | 1st: 36 2nd: Turn 180° | 1st: 367 2nd: Turn 180° | 1st: 27 2nd: Turn 180°
Cylinder head x Cylinder block | 30 | 306 | 22
No. 2 idler gear shaft x Cylinder block | 60 | 612 | 44
Timing chain cover x Cylinder block | 23 | 235 | 17
Water pump x Timing chain cover : for 10 mm head bolt | 9.0 | 92 | 80 in.*lbf
Water pump x Timing chain cover : for 12 mm head bolt | 23 | 235 | 17
Stud bolt x Cylinder block | 4.0 | 41 | 35 in.*lbf
No. 1 oil pan x Cylinder block : for bolt A and B | 21 | 214 | 15
No. 1 oil pan x Cylinder block : for bolt C | 9.0 | 92 | 80 in.*lbf
No. 1 oil pan x Cylinder block : for nut | 21 | 214 | 15
Oil strainer x No. 1 oil pan | 9.0 | 92 | 80 in.*lbf
No. 2 oil pan x No. 1 oil pan | 9.0 | 92 | 80 in.*lbf
No. 2 oil pan x Oil pan drain plug | 40 | 408 | 30
Crankshaft pulley x Crankshaft | 250 | 2,549 | 184
Ventilation valve x Cylinder head cover | 27 | 275 | 20
Oil control valve filter plug x Cylinder head | 62 | 632 | 46
Crankshaft position sensor x Cylinder block | 9.0 | 92 | 80 in.*lbf
VVT sensor x Cylinder head | 8.0 | 82 | 71 in.*lbf
Water drain cook x Cylinder block | 25 | 255 | 18
Oil dipstick guide x Cylinder head | 9.0 | 92 | 80 in.*lbf
No. 1 engine hanger x Cylinder head | 33 | 336 | 24
No. 2 engine hanger x Cylinder head | 33 | 336 | 24