GSIC - Global Service Information Center

# FRONT STABILIZER BAR > INSPECTION

## for Preparation Click here

1. INSPECT FRONT STABILIZER LINK ASSEMBLY LH

1. As shown in the illustration, move the ball joint stud back and forth 5 times before installing the nut.

1. Using a torque wrench, turn the nut continuously at a rate of 3 to 5 seconds per turn and take the torque reading on the fifth turn.

   Turning torque:
     0.05 to 1.96 N*m, (0.5 to 20 kgf*cm, 0.4 to 17 in.*lbf) or less

1. Check for any cracks and grease leaks on the ball joint dust cover.