GSIC - Global Service Information Center

# 2TR-FE COOLING > TORQUE SPECIFICATIONS

Coolant:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Cylinder block drain cock plug x Cylinder block | 24.5 | 250 | 18
  No. 1 engine under cover x Body | 28 | 286 | 21

Water pump:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Water pump assembly x Timing chain cover | for bolt A | 21 | 214 | 155
  for bolt B | 8.9 | 91 | 79 in.*lbf
  V-ribbed belt tensioner Cylinder block | for bolt A | 43 | 439 | 32
  for bolt B | 40 | 408 | 30
  for bolt C | 21 | 214 | 15
  No. 1 idler pulley sub-assembly x Cylinder block | 43 | 439 | 32
  Oil level gauge guide x Cylinder head | 8.0 | 82 | 71 in.*lbf
  Fan shroud x Radiator tank upper | 5.0 | 51 | 44 in.*lbf
  Fluid coupling fan x Water pump assembly | 25 | 255 | 18
  Air pump inlet x Radiator tank lower | 8.5 | 87 | 75 in.*lbf
  No. 1 engine under cover x Body | 28 | 286 | 21

Thermostat:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Water inlet x Cylinder block | 20 | 204 | 15

Fan:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Fan x Fluid coupling | 6.0 | 61 | 53 in.*lbf

Radiator:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Radiator assembly x Body panel | 12 | 122 | 9
  Fan shroud x Radiator tank upper | 5.0 | 51 | 44 in.*lbf
  Fluid coupling fan x Water pump | 25 | 255 | 18
  Air pump inlet x Radiator tank lower | 8.5 | 87 | 75 in.*lbf
  No. 1 engine under cover x Body | 28 | 286 | 21