GSIC - Global Service Information Center

# VACUUM REGULATING VALVE > INSTALLATION

## for Preparation Click here

1. INSTALL VACUUM SWITCHING VALVE (for EGR CUT)

1. Install the valve with the bolt.

   Torque:
     3.5 N*m{ 36 kgf*cm , 31 in.*lbf }

2. INSTALL VACUUM SWITCHING VALVE BRACKET

1. Install the bracket with the 2 bolts.

   Torque:
     20 N*m{ 204 kgf*cm , 15 ft.*lbf }

1. Connect the vacuum hoses to the 3 locations.

1. Connect the 2 connectors.

3. INSTALL NO. 1 ENGINE COVER SUB-ASSEMBLY

1. Install the cover with the 3 bolts and 2 nuts.

   Torque:
     7.0 N*m{ 71 kgf*cm , 62 in.*lbf }

4. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

5. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   CAUTION:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.