GSIC - Global Service Information Center

### BLOWER UNIT > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE INSTRUMENT PANEL SUB-ASSEMBLY UPPER

3. REMOVE INSTRUMENT PANEL SUB-ASSEMBLY LOWER

4. REMOVE NO. 2 HEATER TO REGISTER DUCT

5. REMOVE NO. 1 HEATER TO REGISTER DUCT

6. REMOVE NO. 3 HEATER TO REGISTER DUCT

7. REMOVE NO. 1 INSTRUMENT PANEL BRACE SUB-ASSEMBLY

8. REMOVE NO. 4 AIR DUCT

9. REMOVE STEERING COLUMN ASSEMBLY

10. REMOVE ECM

11. REMOVE INSTRUMENT PANEL REINFORCEMENT

12. REMOVE BLOWER ASSEMBLY