GSIC - Global Service Information Center

### COMMON RAIL > INSTALLATION

1. INSTALL COMMON RAIL ASSEMBLY

2. INSTALL FUEL INLET PIPE SUB-ASSEMBLY

3. INSTALL NO. 2 NOZZLE LEAKAGE PIPE ASSEMBLY

4. INSTALL INJECTION PIPE

5. INSTALL OIL FILTER SUB-ASSEMBLY

6. INSTALL MANIFOLD STAY

7. INSTALL NO. 2 AIR CLEANER PIPE SUB-ASSEMBLY

8. ADD FUEL

9. TIGHTEN FUEL TANK CAP ASSEMBLY

10. ADD ENGINE OIL

11. BLEED AIR FROM FUEL SYSTEM

12. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

13. PERFORM INITIALIZATION

14. CHECK FOR ENGINE OIL LEAKS

15. CHECK FOR FUEL LEAKS

16. INSTALL NO. 2 ENGINE UNDER COVER (for 4WD)

17. INSTALL NO. 1 ENGINE UNDER COVER (for 4WD)