GSIC - Global Service Information Center

# CLUTCH ACCUMULATOR (except 1GR-FE) > INSTALLATION

## for Preparation Click here

1. INSTALL CLUTCH ACCUMULATOR ASSEMBLY

1. Install the clutch accumulator with the 2 nuts.

   Torque:
     18 N*m{ 184 kgf*cm , 13 ft.*lbf }

1. Using SST, connect the 2 flexible tubes.

   SST
     09023-00101

   Torque:
     15 N*m{ 153 kgf*cm , 11 ft.*lbf } for use without SST
     14 N*m{ 143 kgf*cm , 10 ft.*lbf } for use with SST

   HINT:
     Use a torque wrench with a fulcrum length of 30 cm (11.81 in.).

2. BLEED AIR FROM CLUTCH PIPE LINE

1. Fill the master cylinder reservoir with fluid.

   Torque:
     11 N*m{ 112 kgf*cm , 8 ft.*lbf }

1. Bleed air from the clutch system.

3. CHECK FOR CLUTCH FLUID LEAKAGE

1. Check for clutch fluid leakage (Click here).

4. CHECK FOR FLUID LEVEL IN RESERVOIR

1. Check for fluid level in reservoir (Click here).