GSIC - Global Service Information Center

# VACUUM SWITCHING VALVE (for Unleaded Gasoline Specification Vehicle) > INSTALLATION

## for Preparation Click here

1. INSTALL VACUUM SWITCHING VALVE (for EVAP)

1. Install the VSV with the bolt.

   Torque:
     9.0 N*m{ 92 kgf*cm , 80 in.*lbf }

1. Connect the 2 hoses to the VSV.

2. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

3. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   CAUTION:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.