GSIC - Global Service Information Center

# FRONT WIPER MOTOR AND LINK > INSPECTION

## for Preparation Click here

1. REMOVE WINDSHIELD WIPER MOTOR ASSEMBLY (for LHD)

1. Check the LO operation.

   1. Connect the battery's positive (+) lead to terminal 1 (+1) and the negative (-) lead to terminal 5 (E), and check that the motor operates at low speed (LO).

      OK:
        Motor operates at low speed (LO).

1. Check the HI operation.

   1. Connect the battery's positive (+) lead to terminal 4 (+2) and the negative (-) lead to terminal 4 (E), and check that the motor operates at high speed (HI).

      OK:
        Motor operates at high speed (HI).

1. Check the automatic stop operation.

   1. Connect the battery's positive (+) lead to terminal 1 (+1) and the negative (-) lead to terminal 5 (E). With the motor rotating at low speed (LO), disconnect terminal 1 (+1) to stop the wiper motor operation at any position other than the automatic stop position.

   2. Using SST, connect terminals 1 (S) and 1 (+1). Then connect the battery's positive (+) lead to terminal 2 (B) to restart the motor operation at low speed (LO).

      SST
        09843-18040

   3. Check that the motor stops automatically at the automatic stop position.

      OK:
        Refer to illustration on left.
      If the result is not as specified, replace the motor assembly.

2. INSPECT WINDSHIELD WIPER MOTOR ASSEMBLY (for RHD)

1. Check the LO operation.

   1. Connect the battery's positive (+) lead to terminal 5 (+1) and the negative (-) lead to terminal 4 (E), and check that the motor operates at low speed (LO).

      OK:
        Motor operates at low speed (LO).

1. Check the HI operation.

   1. Connect the battery's positive (+) lead to terminal 3 (+2) and the negative (-) lead to terminal 4 (E), and check that the motor operates at high speed (HI).

      OK:
        Motor operates at high speed (HI).

1. Check the automatic stop operation.

   1. Connect the battery's positive (+) lead to terminal 5 (+1) and the negative (-) lead to terminal 4 (E). With the motor rotating at low speed (LO), disconnect terminal 5 (+1) to stop the wiper motor operation at any position other than the automatic stop position.

   2. Using SST, connect terminals 1 (S) and 5 (+1). Then connect the battery's positive (+) lead to terminal 2 (B) to restart the motor operation at low speed (LO).

      SST
        09843-18040

   3. Check that the motor stops automatically at the automatic stop position.

      OK:
        Refer to illustration on left.
      If the result is not as specified, replace the motor assembly.