GSIC - Global Service Information Center

# HOOD > ON-VEHICLE INSPECTION

## for Preparation Click here

1. INSPECT HOOD SUB-ASSEMBLY

1. Check that the clearance measurements of areas A to F are within the standard range.

   Standard:

     Area | Measurement | Area | Measurement
     A (Reference) | 6.0 +- 1.5 mm (0.236 +- 0.059 in.) | D | 0.3 +- 1.5 mm (0.012 +- 0.059 in.)
     B | 0.7 +- 1.5 mm (0.028 +- 0.059 in.) | E (Reference) | 6.0 +- 1.5 mm (0.236 +- 0.059 in.)
     C | 4.0 +- 1.5 mm (0.157 +- 0.059 in.) | F | 0.7 +- 1.5 mm (0.028 +- 0.059 in.)