GSIC - Global Service Information Center

### CRUISE CONTROL SYSTEM > Cruise Main Indicator Light Circuit

## for Preparation Click here

## DESCRIPTION

When the cruise control main switch is turned ON, the CRUISE main indicator light illuminates.

## WIRING DIAGRAM

## INSPECTION PROCEDURE

1.PERFORM ACTIVE TEST (CRUISE MAIN INDICATOR LIGHT)

1. Select the Active Test, use the intelligent tester to generate a control command, and then check that the CRUISE main indicator light illuminates.

   Combination meter assembly:
   Item | Test Details | Diagnostic Note
   Indicator. Light Cruise | CRUISE main indicator light is ON/OFF | -

   OK:
     Cruise main indicator light turns ON/OFF.

| OK |

PROCEED TO NEXT CIRCUIT INSPECTION SHOWN IN PROBLEM SYMPTOMS TABLE

NG |

2.INSPECT FUSE (MET)

1. Remove the MET fuse from the instrument panel junction block.

1. Measure the resistance of the fuse.

   Standard resistance:
     Below 1 Ω

| NG |

REPLACE FUSE

OK |

3.CHECK WIRE HARNESS (COMBINATION METER ASSEMBLY - ECM, BATTERY AND BODY GROUND)

1. Disconnect the E13 or E6 ECM connector.

1. Disconnect the C8 meter connector.

1. Measure the voltage and resistance of the wire harness side connectors.

   Standard voltage:

     Tester Connection | Switch Condition | Specified Condition
     C8-21 - Body ground | Ignition switch ON | 10 to 14 V
     C8-21 - Body ground | Ignition switch OFF | Below 1 V

   Standard resistance:
     1GR-FE:

     Tester Connection | Switch Condition | Specified Condition
     C8-28 - E13-18(PI) | Always | Below 1 Ω
     C8-28 - Body ground | Always | 10 kΩ or higher
     C8-22 - Body ground | Always | Below 1 Ω

     1KD-FTV:

     Tester Connection | Switch Condition | Specified Condition
     C8-28 - E6-3(PI) | Always | Below 1 Ω
     C8-28 - Body ground | Always | 10 kΩ or higher
     C8-22 - Body ground | Always | Below 1 Ω

| NG |

REPAIR OR REPLACE HARNESS AND CONNECTOR

OK |

REPLACE COMBINATION METER ASSEMBLY