GSIC - Global Service Information Center

### POWER WINDOW CONTROL SYSTEM > Front Passenger Side Power Window does not Operate with Front Passenger Side Power Window Switch

## for Preparation Click here

## DESCRIPTION

If the passenger side manual UP / DOWN function does not operate, a malfunction may be present in the power window regulator motor, power window regulator switch, power window regulator master switch or wire harness.

## WIRING DIAGRAM

## INSPECTION PROCEDURE

1.CHECK POWER WINDOW REGULATOR SWITCH ASSEMBLY (PASSENGER SIDE) (POWER SOURCE)

1. Disconnect the P9 regulator switch connector.

1. Measure the voltage of the wire harness side connector.

   Standard voltage:

     Tester Connection | Condition | Specified Condition
     P9-3 - Body ground | Ignition switch ON | 10 to 14 V

| NG |

REPAIR OR REPLACE HARNESS AND CONNECTOR

OK |

2.INSPECT POWER WINDOW REGULATOR SWITCH ASSEMBLY (PASSENGER SIDE)

1. Remove the switch.

1. Measure the resistance of the switch when the switch is operated.

   Standard resistance:

     Tester Connection | Switch Condition | Specified Condition
     5 - 4 2 - 3 | UP | Below 1 Ω
     5 - 4 2 - 1 | OFF | Below 1 Ω
     5 - 3 2 - 1 | DOWN | Below 1 Ω

| NG |

REPLACE POWER WINDOW REGULATOR SWITCH ASSEMBLY (PASSENGER SIDE)

OK |

3.CHECK WIRE HARNESS (SWITCH (PASSENGER SIDE) - MOTOR (PASSENGER SIDE))

1. Disconnect the P9 switch connector.

1. Disconnect the P6*1 or P5*2 motor connector.

1. Measure the resistance of the wire harness side connectors.

   Standard resistance:
     LHD

     Tester Connection | Specified Condition
     P9-5 - P6-1 | Below 1 Ω
     P9-2 - P6-2 | Below 1 Ω
     P9-5 or P6-1 - Body ground | 10 kΩ or higher
     P9-2 or P6-2 - Body ground | 10 kΩ or higher

     RHD

     Tester Connection | Specified Condition
     P9-5 - P5-1 | Below 1 Ω
     P9-2 - P5-2 | Below 1 Ω
     P9-5 or P5-1 - Body ground | 10 kΩ or higher
     P9-2 or P5-2 - Body ground | 10 kΩ or higher

| NG |

REPAIR OR REPLACE HARNESS AND CONNECTOR

OK |

4.INSPECT POWER WINDOW REGULATOR MOTOR ASSEMBLY (PASSENGER SIDE)

1. LHD:

   1. Remove the motor.

   2. Apply battery voltage to connector terminals 1 and 2.

      NOTICE:
        Do not apply battery voltage to any terminals except terminals 1 and 2.

   3. Check that the motor gear rotates smoothly as follows.

      OK:

        Measurement Condition | Specified Condition
        Battery positive (+) → 1 Battery negative (-) → 2 | Motor gear rotates clockwise
        Battery positive (+) → 2 Battery negative (-) → 1 | Motor gear rotates counterclockwise

1. RHD:

   1. Remove the motor.

   2. Apply battery voltage to connector terminals 1 and 2.

      NOTICE:
        Do not apply battery voltage to any terminals except terminals 1 and 2.

   3. Check that the motor gear rotates smoothly as follows.

      OK:

        Measurement Condition | Specified Condition
        Battery positive (+) → 1 Battery negative (-) → 2 | Motor gear rotates counterclockwise
        Battery positive (+) → 2 Battery negative (-) → 1 | Motor gear rotates clockwise

| NG |

REPLACE POWER WINDOW REGULATOR MOTOR ASSEMBLY (PASSENGER SIDE)

OK |

5.CHECK WIRE HARNESS (MASTER SWITCH - SWITCH (PASSENGER SIDE))

1. LHD:

   1. Disconnect the P4 master switch connector.

   2. Disconnect the P9 switch connector.

   3. Measure the resistance of the wire harness side connectors.

      Standard resistance:
        Single cab, Extra cab

        Tester Connection | Specified Condition
        P4-8 (PU) - P9-1 | Below 1 Ω
        P4-10 (PD) - P9-4 | Below 1 Ω
        P4-8 (PU) or P9-1 - Body ground | 10 kΩ or higher
        P4-10 (PD) or P9-4 - Body ground | 10 kΩ or higher

        Double cab

        Tester Connection | Specified Condition
        P4-18 (PU) - P9-1 | Below 1 Ω
        P4-15 (PD) - P9-4 | Below 1 Ω
        P4-18 (PU) or P9-1 - Body ground | 10 kΩ or higher
        P4-15 (PD) or P9-4 - Body ground | 10 kΩ or higher

1. RHD:

   1. Disconnect the P4 master switch connector.

   2. Disconnect the P9 switch connector.

   3. Measure the resistance of the wire harness side connectors.

      Standard resistance:
        Single cab, Extra cab

        Tester Connection | Specified Condition
        P4-8 (PU) - P9-1 | Below 1 Ω
        P4-1 (PD) - P9-4 | Below 1 Ω
        P4-8 (PU) or P9-1 - Body ground | 10 kΩ or higher
        P4-1 (PD) or P9-4 - Body ground | 10 kΩ or higher

        Double cab

        Tester Connection | Specified Condition
        P4-10 (PU) - P9-1 | Below 1 Ω
        P4-13 (PD) - P9-4 | Below 1 Ω
        P4-10 (PU) or P9-1 - Body ground | 10 kΩ or higher
        P4-13 (PD) or P9-4 - Body ground | 10 kΩ or higher

| NG |

REPAIR OR REPLACE HARNESS AND CONNECTOR

OK |

6.INSPECT POWER WINDOW REGULATOR MASTER SWITCH ASSEMBLY (FRONT PASSENGER SWITCH)

1. LHD (Single cab, extra cab):
   Inspect the front passenger switch.

   1. Remove the master switch.

   2. Measure the resistance of the switch when the switch is operated.

      Standard resistance:

        Window Lock Switch Condition | Power Window Switch Condition | Tester Connection | Specified Condition
        OFF | UP | 1 (E) - 10 (PD) 8 (PU) - 9 (B) | Below 1 Ω
        OFF | OFF | 1 (E) - 8 (PU) 1 (E) - 10 (PD) | Below 1 Ω
        OFF | DOWN | 1 (E) - 8 (PU) 9 (B) - 10 (PD) | Below 1 Ω
        ON | UP | 1 (E) - 10 (PD) | 10 kΩ or higher
        8 (PU) - 9 (B) | Below 1 Ω
        ON | OFF | 8 (PU) - 10 (PD) | Below 1 Ω
        ON | DOWN | 1 (E) - 8 (PU) | 10 kΩ or higher
        9 (B) - 10 (PD) | Below 1 Ω

1. RHD (Single cab, extra cab):
   Inspect the front passenger switch.

   1. Remove the master switch.

   2. Measure the resistance of the switch when the switch is operated.

      Standard resistance:

        Window Lock Switch Condition | Power Window Switch Condition | Tester Connection | Specified Condition
        OFF | UP | 1 (PD) - 10 (E) 8 (PU) - 9 (B) | Below 1 Ω
        OFF | OFF | 8 (PU) - 10 (E) 1 (PD) - 10 (E) | Below 1 Ω
        OFF | DOWN | 8 (PU) - 10 (E) 1 (PD) - 9 (B) | Below 1 Ω
        ON | UP | 1 (PD) - 10 (E) | 10 kΩ or higher
        8 (PU) - 9 (B) | Below 1 Ω
        ON | OFF | 1 (PD) - 8 (PU) | Below 1 Ω
        ON | DOWN | 8 (PU) - 10 (E) | 10 kΩ or higher
        1 (PD) - 9 (B) | Below 1 Ω

1. LHD (Double cab):
   Inspect the front passenger switch.

   1. Remove the master switch.

   2. Measure the resistance of the switch when the switch is operated.

      Standard resistance:

        Window Lock Switch Condition | Power Window Switch Condition | Tester Connection | Specified Condition
        OFF | UP | 3 (E) - 15 (PD) 6 (B) - 18 (PU) | Below 1 Ω
        OFF | OFF | 3 (E) - 18 (PU) 3 (E) - 15 (PD) | Below 1 Ω
        OFF | DOWN | 3 (E) - 18 (PU) 6 (B) - 15 (PD) | Below 1 Ω
        ON | UP | 3 (E) - 15 (PD) | 10 kΩ or higher
        6 (B) - 18 (PU) | Below 1 Ω
        ON | OFF | 15 (PD) - 18 (PU) | Below 1 Ω
        ON | DOWN | 3 (E) - 18 (PU) | 10 kΩ or higher
        6 (B) - 15 (PD) | Below 1 Ω

1. RHD (Double cab):
   Inspect the front passenger switch.

   1. Remove the master switch.

   2. Measure the resistance of the switch when the switch is operated.

      Standard resistance:

        Window Lock Switch Condition | Power Window Switch Condition | Tester Connection | Specified Condition
        OFF | UP | 3 (E) - 13 (PD) 6 (B) - 10 (PU) | Below 1 Ω
        OFF | OFF | 3 (E) - 10 (PU) 3 (E) - 13 (PD) | Below 1 Ω
        OFF | DOWN | 3 (E) - 10 (PU) 6 (B) - 13 (PD) | Below 1 Ω
        ON | UP | 3 (E) - 13 (PD) | 10 kΩ or higher
        6 (B) - 10 (PU) | Below 1 Ω
        ON | OFF | 10 (PU) - 13 (PD) | Below 1 Ω
        ON | DOWN | 3 (E) - 10 (PU) | 10 kΩ or higher
        6 (B) - 13 (PD) | Below 1 Ω

| NG |

REPLACE POWER WINDOW REGULATOR MASTER SWITCH ASSEMBLY

OK |

GO TO POWER WINDOWS DO NOT OPERATE AT ALL