GSIC - Global Service Information Center

# HEADLIGHT ASSEMBLY > INSTALLATION

## for Preparation Click here

1. INSTALL CLEARANCE LIGHT BULB

1. Turn the bulb in the direction indicated by the arrow to install it.

2. INSTALL FRONT TURN SIGNAL LIGHT BULB

1. Install the bulb to the socket.

1. Turn the bulb/socket unit in the direction indicated by the arrow to install it.

3. INSTALL NO. 1 HEADLIGHT BULB

1. Release the lock of the set spring and install the bulb.

4. INSTALL HEADLIGHT SOCKET COVER

5. INSTALL HEADLIGHT ASSEMBLY LH

1. Connect the connectors and install the headlight.

1. Install the 3 screws and bolts.

6. INSTALL FRONT BUMPER COVER

1. Put protective tape under the front fender.

1. Attach the 4 claws to install the cover.

1. Install the 9 clips.

7. INSTALL ENGINE SIDE COVER SUB-ASSEMBLY LH

1. Install the engine side cover with the 3 bolts and 2 clips.

8. INSTALL ENGINE SIDE COVER SUB-ASSEMBLY RH

9. INSTALL FRONT FENDER LINER LH

1. Install the fender liner with the 3 clips and screw.

10. INSTALL RADIATOR GRILLE

1. Push the radiator grille in the direction indicated by the arrow in the illustration. Attach the 5 claws to install the radiator grille.

1. Install the 2 screws and 2 clips.

11. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

12. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.

13. ADJUST HEADLIGHT AIMING

1. Adjust the headlight aiming (Click here ).