GSIC - Global Service Information Center

# REAR DOOR BELT MOULDING > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE REAR DOOR WINDOW REGULATOR HANDLE ASSEMBLY (w/o Power Window)

3. REMOVE DOOR PULL HANDLE

4. REMOVE REAR DOOR ARMREST BASE PANEL UPPER LH (w/ Power Window)

5. REMOVE REAR DOOR TRIM BOARD SUB-ASSEMBLY LH

6. REMOVE REAR DOOR BELT MOULDING ASSEMBLY LH

1. Put protective tape under the moulding.

1. Using a moulding remover, pry out the moulding as shown in the illustration.

   HINT:
     Tape the remover tip before use.

   NOTICE:
     Be careful when removing the moulding as there are claws attached to the the moulding.