GSIC - Global Service Information Center

# ACCELERATOR PEDAL ROD > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE ACCELERATOR PEDAL ROD

1. Disconnect the accelerator pedal position sensor connector.

1. Remove the 2 bolts and accelerator pedal rod.

   NOTICE:
   1. Do not drop or strike the accelerator pedal rod.
   2. Do not disassemble the accelerator pedal rod.