GSIC - Global Service Information Center

# OUTSIDE MOULDING > REMOVAL

## for Preparation Click here

1. REMOVE FRONT WHEEL OPENING EXTENSION SUB-ASSEMBLY LH

1. Remove the 7 screws.

1. Detach the 8 clips and remove the extension.

2. REMOVE FRONT WHEEL OPENING EXTENSION SUB-ASSEMBLY RH

HINT:

  Use the same procedures described for the LH side.

3. REMOVE NO. 1 REAR WHEEL OPENING EXTENSION LH

1. Remove the 7 screws.

1. Detach the 11 clips and remove the extension.

4. REMOVE NO. 1 REAR WHEEL OPENING EXTENSION RH

1. Remove the 7 screws.

1. Detach the 12 clips and remove the extension.