GSIC - Global Service Information Center

# DIESEL THROTTLE BODY > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag activation.

2. REMOVE NO. 2 AIR CLEANER PIPE SUB-ASSEMBLY

1. Disconnect the manifold absolute pressure sensor connector.

1. Disconnect the vacuum hose from the gas filter.

1. Loosen the 2 clamps.

1. Remove the bolt and disconnect the pipe together with the 2 air hoses.

3. REMOVE DIESEL THROTTLE BODY ASSEMBLY

1. Disconnect the 2 connectors.

1. Remove the 2 bolts, 2 nuts, throttle body and gasket.