GSIC - Global Service Information Center

# CLUTCH PEDAL (for RHD) > DISASSEMBLY

## for Preparation Click here

1. REMOVE CLUTCH PEDAL SPRING (w/ Turn over)

1. Remove the clutch pedal spring.

2. REMOVE CLUTCH PEDAL SUB-ASSEMBLY

1. w/ Turn over:
   Remove the clutch pedal return spring.

1. Remove the bolt, nut and clutch pedal from the clutch pedal support.

3. REMOVE CLUTCH PEDAL SPRING HOLDER (w/ Turn over)

1. Remove the clutch pedal spring holder.

4. REMOVE COLLAR

1. Remove the 2 bushes and collar.

5. REMOVE NO. 1 CLUTCH PEDAL CUSHION

1. Remove the cushion from the clutch pedal.

6. REMOVE CLUTCH PEDAL TURN OVER BUSH (w/ Turn over)

1. Remove the bush from the clutch pedal support.

7. REMOVE PEDAL SPRING HOOK (w/ Turn over)

1. Remove the hook from the clutch pedal support.