GSIC - Global Service Information Center

# OIL PUMP > REASSEMBLY

## for Preparation Click here

1. INSTALL FRONT OIL PUMP OIL SEAL

1. Using SST and a hammer, install a new oil seal.

   SST
     09350-30020 (09351-32140)

   HINT:
     The oil seal end should be flush with the outer edge of the pump body.

1. Coat the oil seal lip with MP grease.

2. FIX FRONT OIL PUMP BODY SUB-ASSEMBLY

1. Place the oil pump body on the torque converter clutch.

3. INSTALL FRONT OIL PUMP DRIVEN GEAR

1. Coat the driven gear with ATF.

1. Install the driven gear to the oil pump body.

4. INSTALL FRONT OIL PUMP DRIVE GEAR

1. Coat the drive gear with ATF.

1. Install the drive gear to the oil pump body.

5. INSTALL FRONT OIL PUMP BODY O-RING

1. Install the O-ring to the oil pump body.

6. INSTALL STATOR SHAFT ASSEMBLY

1. Install the stator shaft with each bolt hole.

1. Install the 14 bolts.

   Torque:
     12 N*m{ 122 kgf*cm , 9 ft.*lbf }

7. INSTALL CLUTCH DRUM OIL SEAL RING

1. Coat the 3 oil seal rings with ATF.

1. Squeeze the ends of the 3 oil seal rings together with the overlap distance 8 mm (0.314 in.) or less, and then install them to the starter shaft groove.

   NOTICE:
     Do not over-spread the ring ends.

   HINT:
     After installing the oil seal rings, check that they rotate smoothly.

8. INSPECT OIL PUMP DRIVE GEAR ROTATION

1. Make sure the drive gear rotates smoothly.

1. Remove the oil pump assembly from the torque converter.

9. INSTALL FRONT OIL PUMP BODY O-RING

1. Install the O-ring to the oil pump assembly.