GSIC - Global Service Information Center

# INJECTOR DRIVER > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE INJECTOR DRIVER

1. Disconnect the 2 connectors.

1. Remove the 2 bolts and injector driver.

3. REMOVE INJECTOR DRIVER BRACKET

1. Remove the 3 screws and driver bracket.