GSIC - Global Service Information Center

# FAN > INSTALLATION

## for Preparation Click here

1. INSTALL FAN

1. Install the fan to the coupling with the 4 nuts.

   Torque:
     6.0 N*m{ 61 kgf*cm , 53 in.*lbf }

2. INSTALL FAN SHROUD

1. Install the fan pulley to the water pump.

1. Install the shroud together with the coupling fan between the radiator and engine component.

   NOTICE:
     Be careful not to damage the radiator core.

1. Install the fluid coupling fan to the fan pulley with the 4 nuts.
   Tighten the nuts as much as possible by hand.

1. Attach the shroud's claws to the radiator.

1. Install the shroud with the 2 bolts.

   Torque:
     5.0 N*m{ 51 kgf*cm , 44 in.*lbf }

1. Install the drive belt (Click here).

1. Tighten the 4 nuts of the fluid coupling fan.

   Torque:
     18 N*m{ 184 kgf*cm , 13 ft.*lbf }

1. Install the radiator reservoir with the 2 bolts.

   Torque:
     5.0 N*m{ 51 kgf*cm , 44 in.*lbf }

1. Connect the No. 1 and No. 2 water by-pass hoses to the tank upper and lower.

1. Install the oil reservoir with the 3 bolts.

   Torque:
     5.0 N*m{ 51 kgf*cm , 44 in.*lbf }

3. CONNECT RADIATOR HOSE INLET

4. ADD ENGINE COOLANT

1. Add the engine coolant (Click here).

5. CHECK FOR ENGINE COOLANT LEAKS

1. Check for the engine coolant leaks (Click here).

6. INSTALL NO. 1 ENGINE UNDER COVER

1. Install the cover with the 4 bolts.

   Torque:
     28 N*m{ 286 kgf*cm , 21 ft.*lbf }