GSIC - Global Service Information Center

# FRONT BRAKE (for 4WD) > REMOVAL

## for Preparation Click here

HINT:

1. Use the same procedures for the LH side and RH side.
2. The procedures listed below are for the LH side.

1. REMOVE FRONT WHEEL

2. DRAIN BRAKE FLUID

NOTICE:

  Wash off brake fluid immediately if it comes in contact with any painted surface.

3. REMOVE FRONT DISC BRAKE ANTI-RATTLE SPRING

1. Remove the clip.

1. Hold down the spring and remove the 2 pins.

1. Remove the spring.

   CAUTION:
     Do not remove the 2 pins without holding down the spring. The spring will eject with a force capable of causing injury.

4. REMOVE FRONT DISC BRAKE PAD

1. Remove the 2 disc brake pads.

5. REMOVE FRONT ANTI SQUEAL SHIM KIT

1. Remove the No.1 and No. 2 shims from each pad.

6. DISCONNECT FRONT NO. 1 WHEEL CYLINDER TUBE LH

1. Using SST, disconnect the tube from the cylinder.

   SST
     09023-00101

7. REMOVE DISC BRAKE CYLINDER ASSEMBLY LH

1. Remove the 2 bolts and cylinder.