GSIC - Global Service Information Center

### CAMSHAFT (for Bank 1) > REMOVAL

1. DISCONNECT BATTERY NEGATIVE TERMINAL

2. DISCHARGE FUEL SYSTEM PRESSURE

3. DRAIN ENGINE COOLANT

4. REMOVE DRIVE BELT

5. REMOVE V-BANK COVER

6. REMOVE NO. 2 VENTILATION HOSE

7. REMOVE AIR CLEANER

8. REMOVE INTAKE AIR SURGE TANK

9. REMOVE IGNITION COIL

10. REMOVE CYLINDER HEAD COVER RH

11. REMOVE CYLINDER HEAD COVER LH

12. SET NO. 1 CYLINDER TO TDC/COMPRESSION

13. REMOVE NO. 1 CHAIN TENSIONER

14. REMOVE NO. 2 CAMSHAFT

15. REMOVE NO. 2 CHAIN TENSIONER

16. REMOVE NO. 1 CAMSHAFT