GSIC - Global Service Information Center

# RADIO RECEIVER > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE HEATER CONTROL KNOB

1. Remove the 3 control knobs.

3. REMOVE FRE/REC CONTROL KNOB

1. Remove the control knob.

4. REMOVE INSTRUMENT CLUSTER FINISH PANEL ASSEMBLY CENTER

HINT:

  To prevent the clips from falling, horizontally pull out the panel. Hold both sides of the panel in the locations indicated by the arrows in the illustration.

1. Remove the screw <C>.

1. Detach the 6 claws and 4 clips.

1. NOTICE:
     Make sure the center registers are not removed.
   Disconnect all connectors and remove the panel.

5. REMOVE RADIO RECEIVER ASSEMBLY WITH BRACKET

1. Remove the 4 screws.

1. Disconnect all connectors and remove the radio receiver.

1. w/o Stereo opening cover:
   Remove the No. 1 radio bracket.

   1. Remove the 4 screws and radio bracket from the radio receiver.

1. w/o Stereo opening cover:
   Remove the No. 2 radio bracket.

   1. Remove the 4 screws and radio bracket from the radio receiver.

1. w/ Stereo opening cover:
   Remove the No. 1 radio bracket.

   1. Remove the 4 screws and radio bracket from the radio receiver.

1. w/ Stereo opening cover:
   Remove the No. 2 radio bracket.

   1. Remove the 4 screws and radio bracket from the radio receiver.