GSIC - Global Service Information Center

# CHARGING SYSTEM > PRECAUTION

## for Preparation Click here

1.Check that the battery cables are connected to the correct terminals.

2.Disconnect the battery cables when the battery is quickly charged.

3.Do not perform tests with a high voltage insulation resistance tester.

4.Never disconnect the battery cable while the engine is running.

5.Check that the charging cable nut is tightened on terminal B of the generator and the fuse box.

6.If the generator is installed to the vehicle, do not perform checks on terminal F.