GSIC - Global Service Information Center

### WATER PUMP > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE NO. 1 ENGINE UNDER COVER

3. DRAIN ENGINE COOLANT

4. DISCONNECT RADIATOR HOSE INLET

5. REMOVE FAN SHROUD

6. REMOVE COOLER COMPRESSOR ASSEMBLY

7. REMOVE GENERATOR ASSEMBLY

8. REMOVE V-RIBBED BELT TENSIONER ASSEMBLY

9. REMOVE CHARGE AIR COOLER ASSEMBLY

10. REMOVE NO. 1 TIMING BELT COVER

11. REMOVE TIMING BELT

12. REMOVE NO. 1 TIMING BELT IDLER SUB-ASSEMBLY

13. REMOVE INJECTION PIPE

14. REMOVE CYLINDER HEAD COVER SUB-ASSEMBLY

15. CLEAN CAMSHAFT TIMING PULLEY

16. REMOVE NO. 2 TIMING BELT COVER

17. REMOVE WATER PUMP ASSEMBLY