GSIC - Global Service Information Center

# FRONT STABILIZER BAR > REMOVAL

## for Preparation Click here

HINT:

1. Use the same procedures for the RH side and LH side.

1. The procedures listed below are for the LH side.

1. A bolt without a torque specification is shown in the standard bolt chart.

1. REMOVE FRONT WHEEL

2. REMOVE FRONT STABILIZER LINK ASSEMBLY LH

1. Remove the 2 nuts and stabilizer link.

   HINT:
     If the ball joint turns together with the nut, use a 6 mm hexagon wrench to hold the stud in place.

3. REMOVE FRONT STABILIZER LINK ASSEMBLY RH

HINT:

  Use the same procedures described for the LH side.

4. REMOVE FRONT STABILIZER BRACKET

1. Remove the 4 bolts and 2 brackets.

5. REMOVE FRONT NO. 1 STABILIZER BAR BUSH

1. Remove the 2 bushes.

6. REMOVE FRONT STABILIZER BAR

1. Remove the stabilizer bar front from the vehicle body.