GSIC - Global Service Information Center

# 2KD-FTV STARTING > SERVICE DATA

Starter | Rated voltage and output power 12 V 2.0 kW No-load characteristics current 100 A or less at 11.5 V
Glow plug | Resistance Approx. 0.95 Ω

ECT sensor

Resistance
Approx. 20 °C (68°F)
2.32 to 2.59 kΩ
Approx. 20 °C (68°F)
0.310 to 0.326 kΩ

Starter relay

3 - 5
Specified resistance
10 MΩ or higher
Below 1 Ω
(when battery voltage is applied to terminals 1 and 2)

Glow relay

3 - 5
Specified resistance
10 MΩ or higher
Below 1 Ω
(when battery voltage is applied to terminals 1 and 2)

Ignition switch

Tester connection
-
Switch condition
LOCK
Specified condition
10 kΩ or higher

Tester connection
2 (ACC) - 4 (AM1)
Switch condition
ACC
Specified condition
Below 1 Ω

Tester connection
1 (IG1) - 4 (AM1)
2 (ACC) - 4 (AM1)
5 (AM2) - 6 (IG2)
Switch condition
ON
Specified condition
Below 1 Ω

Tester connection
1 (IG1) - 4 (AM1)
2 (ACC) - 4 (AM1)
5 (AM2) - 6 (IG2)
5 (AM2) - 7 (ST2)
Switch condition
START
Specified condition
Below 1 Ω