GSIC - Global Service Information Center

# VALVE BODY > REASSEMBLY

## for Preparation Click here

1. INSTALL TRANSMISSION SOLENOID ASSEMBLY

1. Install the shift solenoid valve SL with the bolt.

   Torque:
     10 N*m{ 100 kgf*cm , 7 ft.*lbf }

1. Install the shift solenoid valve S1 and S2 with the bolt.

   Torque:
     6.6 N*m{ 67 kgf*cm , 56 in.*lbf }

1. Install the shift solenoid valve SLT with the plate and bolt.

   Torque:
     6.4 N*m{ 65 kgf*cm , 56 in.*lbf }

2. INSTALL TRANSMISSION VALVE BODY ASSEMBLY

1. Align the groove of the manual valve with the pin of the lever.

1. Install the 20 bolts.

   Torque:
     10 N*m{ 100 kgf*cm , 7 ft.*lbf }

   HINT:
     Bolt length:
     23 mm (0.91 in.) for A
     28 mm (1.10 in.) for B
     36 mm (1.42 in.) for C