GSIC - Global Service Information Center

# FRONT PASSENGER SIDE POWER WINDOW SWITCH > ON-VEHICLE INSPECTION

## for Preparation Click here

1. INSPECT POWER WINDOW REGULATOR SWITCH ASSEMBLY

1. Measure the resistance of the switch when the switch is operated.

   Standard resistance:

     Tester Connection | Switch Condition | Specified Condition
     5 - 4 2 - 3 | UP | Below 1 Ω
     5 - 4 2 - 1 | OFF | Below 1 Ω
     5 - 3 2 - 1 | DOWN | Below 1 Ω

   1. If the result is not as specified, replace the regulator switch assembly.