GSIC - Global Service Information Center

# FRONT SPEED SENSOR > REMOVAL

## for Preparation Click here

HINT:

1. Use the same procedures for the LH side and RH side.
2. The procedures listed below are for the LH side.

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE FRONT WHEEL

3. REMOVE FRONT SPEED SENSOR LH (2WD)

1. Disconnect the sensor connector labeled A.

1. Disconnect the 4 clamps labeled B.

1. Remove the 4 bolts labeled C and disconnect the 4 brackets.

1. Remove the bolt labeled D and sensor.

   NOTICE:
     Keep the sensor tip and sensor installation hole free from foreign matter.

4. REMOVE FRONT SPEED SENSOR LH (4WD)

1. Disconnect the sensor connector labeled A.

1. Disconnect the 6 clamps labeled B.

1. Remove the 3 bolts labeled C and disconnect the 3 brackets.

1. Disconnect the 2 clamps labeled D.

1. Remove the bolt labeled E and sensor.

   NOTICE:
     Keep the sensor tip and sensor installation hole free from foreign matter.