GSIC - Global Service Information Center

# FRONT SHOCK ABSORBER WITH COIL SPRING (for 2WD) > DISASSEMBLY

## for Preparation Click here

1. REMOVE FRONT SUPPORT TO FRONT SHOCK ABSORBER NUT

1. Using SST, compress the coil spring.

   SST
     09710-22021 (09710-01071, 09710-01081)

   NOTICE:
     Do not use an impact wrench. It will damage SST.

1. Hold the shock absorber rod and remove the nut.

   NOTICE:
     Do not use an impact wrench. It will damage the shock absorber rod.

2. REMOVE FRONT SHOCK ABSORBER CUSHION RETAINER

1. Remove the cushion retainer from the shock absorber.

3. REMOVE FRONT SHOCK ABSORBER CUSHION

1. Remove the cushion from the shock absorber.

4. REMOVE FRONT SUSPENSION SUPPORT SUB-ASSEMBLY LH

1. Remove the suspension support from the shock absorber.

5. REMOVE FRONT COIL SPRING INSULATOR UPPER LH

1. Remove the insulator upper from the coil spring.

6. REMOVE FRONT COIL SPRING LH

1. Remove the coil spring from the shock absorber.