GSIC - Global Service Information Center

### FRONT AXLE HUB (for 2WD) > REMOVAL

1. REMOVE FRONT WHEEL

2. REMOVE FRONT SPEED SENSOR LH

3. REMOVE FRONT DISC BRAKE CALIPER ASSEMBLY LH

4. REMOVE FRONT DISC

5. DISCONNECT TIE ROD END SUB-ASSEMBLY

6. DISCONNECT FRONT SUSPENSION LOWER ARM ASSEMBLY WITH ATTACHMENT LH

7. DISCONNECT FRONT SUSPENSION UPPER ARM ASSEMBLY LH

8. REMOVE FRONT AXLE HUB ASSEMBLY

9. REMOVE KNUCKLE GREASE RETAINER CAP

10. REMOVE FRONT AXLE HUB NUT AND SPACER

11. REMOVE STEERING KNUCKLE

12. REMOVE FRONT AXLE HUB OIL SEAL

13. REMOVE FRONT AXLE HUB INNER BEARING