GSIC - Global Service Information Center

# KNOCK SENSOR > INSTALLATION

## for Preparation Click here

1. INSTALL KNOCK SENSOR

1. Install the 2 knock sensors with the 2 bolts as shown in the illustration.

   Torque:
     20 N*m{ 204 kgf*cm , 15 ft.*lbf }

1. Connect the 2 knock sensor connectors.

2. INSTALL CYLINDER HEAD SUB-ASSEMBLY

1. Install the cylinder head (Click here).

3. INSTALL ENGINE ASSEMBLY

1. Install the engine assembly (Click here).

4. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

5. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.