GSIC - Global Service Information Center

# FAN > REMOVAL

## for Preparation Click here

1. REMOVE NO. 1 ENGINE UNDER COVER

1. Remove the 4 bolts and under cover.

2. DRAIN ENGINE COOLANT

1. Remove the radiator cap.

1. Loosen the 2 cylinder block drain cock plugs and radiator drain plug, and then the coolant.

   HINT:
     Collect the coolant in a container and dispose of it according to the regulations in your area.

3. DISCONNECT RADIATOR HOSE INLET

4. DISCONNECT RADIATOR HOSE OUTLET

5. REMOVE FAN SHROUD

1. Disconnect the radiator reservoir hose from the radiator tank upper.

1. Loosen the 4 nuts holding the fluid coupling fan.

1. Remove the driver belt (Click here).

1. Remove the 2 bolts holding the fan shroud.

1. Remove the 4 nuts of the fluid coupling fan, and then remove the shroud together with the coupling fan.

   NOTICE:
     Be careful not to damage the radiator core.

1. Remove the fan pulley from the water pump.

6. REMOVE FAN

1. Remove the 4 nuts and fan from the fluid coupling.