GSIC - Global Service Information Center

# AIR CONDITIONING SWITCH > INSTALLATION

## for Preparation Click here

1. INSTALL A/C SWITCH

1. Install the switch to attach the 2 claws.

2. INSTALL INSTRUMENT CLUSTER FINISH PANEL ASSEMBLY CENTER

1. Connect all connectors.

1. Attach the 6 claws and 4 clips to install the panel.

1. Install the panel with the screw <C>.

3. INSTALL FRE/REC CONTROL KNOB

1. Install the control knob.

4. INSTALL HEATER CONTROL KNOB

1. Install the 3 control knobs.

5. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

6. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.