GSIC - Global Service Information Center

### REAR DIFFERENTIAL CARRIER OIL SEAL > REPLACEMENT

1. REMOVE REAR PROPELLER SHAFT ASSEMBLY

2. REMOVE REAR DRIVE PINION NUT

3. REMOVE REAR DRIVE PINION COMPANION FLANGE SUB-ASSEMBLY

4. REMOVE REAR DIFFERENTIAL CARRIER OIL SEAL

5. REMOVE REAR DIFFERENTIAL DRIVE PINION OIL SLINGER

6. REMOVE REAR DRIVE PINION FRONT TAPERED ROLLER BEARING

7. REMOVE DIFFERENTIAL OIL STORAGE RING

8. REMOVE REAR DIFFERENTIAL DRIVE PINION BEARING SPACER

9. INSTALL REAR DIFFERENTIAL DRIVE PINION BEARING SPACER

10. INSTALL DIFFERENTIAL OIL STORAGE RING

11. INSTALL REAR DRIVE PINION FRONT TAPERED ROLLER BEARING

12. INSTALL REAR DIFFERENTIAL DRIVE PINION OIL SLINGER

13. INSTALL REAR DIFFERENTIAL CARRIER OIL SEAL

14. INSTALL REAR DRIVE PINION COMPANION FLANGE SUB-ASSEMBLY

15. INSPECT DIFFERENTIAL DRIVE PINION PRELOAD

16. STAKE DRIVE PINION NUT

17. INSTALL REAR PROPELLER SHAFT ASSEMBLY

18. REFILL DIFFERENTIAL OIL

19. CHECK FOR DIFFERENTIAL OIL LEAKAGE