GSIC - Global Service Information Center

### DTC 63-45 Eject Error

## for Preparation Click here

## DESCRIPTION

DTC No. | DTC Detection Condition | Trouble Area

63-45

Magazine cannot be ejected.

1. CD
2. Radio receiver assembly

## INSPECTION PROCEDURE

1.PRESS "EJECT" AND CHECK OPERATION

1. Press the CD EJECT switch of the radio receiver for 2 seconds or more and check that the CD ejects.

   OK:
     CD ejects.

| NG |

REPLACE RADIO RECEIVER ASSEMBLY

OK |

2.REPLACE CD WITH ANOTHER AND RECHECK

1. Replace the CD with a normal CD and check that the CD ejects.

   OK:
     CD ejects.

| NG |

REPLACE RADIO RECEIVER ASSEMBLY

OK |

CD IS FAULTY