GSIC - Global Service Information Center

# 2KD-FTV ENGINE CONTROL SYSTEM > SERVICE DATA

Engine coolant temperature sensor | Resistance 2.32 to 2.59 kΩ at 20°C (68°F) 0.310 to 0.326 kΩ at 80°C (176°F)
Intake air temperature sensor | Resistance 2.21 to 2.65 kΩ at 20°C (68°F)
Crankshaft position sensor | Resistance 1,850 to 2,450 Ω at 20°C (68°F)
Camshaft position sensor | Resistance 950 to 1,250 Ω at 20°C (68°F)
Integration relay (EDU relay) | Specified condition IJ-8 -Body ground at ignition switch ON 10 to 14 V
Integration relay (MAIN relay) | Specified condition IJ-4 -Body ground at ignition switch ON 10 to 14 V