GSIC - Global Service Information Center

# ROOF HEADLINING (for Single Cab) > INSTALLATION

## for Preparation Click here

1. INSTALL NO. 2 SIDE RAIL SPACER REAR LH

2. INSTALL NO. 2 SIDE RAIL SPACER REAR RH

3. INSTALL SIDE RAIL SPACER REAR LH (for LHD)

4. INSTALL SIDE RAIL SPACER REAR RH (for RHD)

5. INSTALL SIDE RAIL SPACER FRONT LH

6. INSTALL SIDE RAIL SPACER FRONT RH

7. INSTALL ROOF NO. 2 SILENCER PAD

8. INSTALL ROOF HEADLINING ASSEMBLY

1. Align the wire harness to the markings, and then install the wire harness with tape.

   NOTICE:
     Attach the roof wire harness securely.

1. Install the roof headlining with the 5 clips.

9. INSTALL ASSIST GRIP

1. Install the assist grip with the 2 screws.

1. Close the 2 covers.

10. INSTALL VISOR HOLDER LH

1. Attach the 2 claws to install the holder.

1. Install the screw.

11. INSTALL VISOR HOLDER RH

HINT:

  Use the same procedures described for the LH side.

12. INSTALL VISOR ASSEMBLY LH

1. Install the visor with the screw.

13. INSTALL VISOR ASSEMBLY RH

1. Install the visor with the screw.

14. INSTALL ROOM LIGHT ASSEMBLY

Click here

15. INSTALL BACK PANEL TRIM (w/ Back Panel Trim)

1. Install the back panel trim with the 3 clips.

16. INSTALL QUARTER INSIDE TRIM BOARD LH

1. Attach the 3 clips to install the trim board.

17. INSTALL QUARTER INSIDE TRIM BOARD RH

HINT:

  Use the same procedures described for the LH side.

18. INSTALL QUARTER TRIM PANEL LOWER LH

1. Attach the 3 clips and claw to install the trim panel.

19. INSTALL QUARTER TRIM PANEL LOWER RH

HINT:

  Use the same procedures described for the LH side.

20. INSTALL FRONT SEAT OUTER BELT ASSEMBLY LH

NOTICE:

  Do not disassemble the retractor.

1. w/o Pretensioner single cab and extra cab:
   Align the claws with the seat belt positioning holes and install the ELR of the seat belt with the bolt as shown in the illustration.

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf }

1. w/o Pretensioner Double cab:
   Align the claws with the seat belt positioning holes and install the ELR of the seat belt with the bolt as shown in the illustration.

   Torque:
     4.8 N*m{ 49 kgf*cm , 42 in.*lbf }

1. w/ Pretensioner:
   Install the bolt and seat belt.

   Torque:
     4.8 N*m{ 49 kgf*cm , 42 in.*lbf } for bolt A

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf } for bolt B

1. w/ Pretensioner:
   Connect the pretensioner connector as shown in the illustration.

1. Single cab:
   Install the anchor with the bolt.

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf }

1. Close the cover.

1. Extra cab and double cab:
   Install the anchor with the bolt.

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf }

1. Install the cap.

1. Single cab:
   Install the quarter trim panel lower. Then install the seat belt floor anchor with the bolt.

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf }

1. Extra cab:
   Install the quarter inside trim board. Then install the seat belt floor anchor with the bolt.

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf }

1. Double cab:
   Install the anchor of the seat belt with the built-in bolt after installing the center pillar garnish lower.

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf }

21. INSTALL FRONT SEAT OUTER BELT ASSEMBLY RH

NOTICE:

  Do not disassemble the retractor.

1. w/o Pretensioner single cab and extra cab:
   Align the claws with the seat belt positioning holes and install the ELR of the seat belt with the bolt as shown in the illustration.

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf }

1. w/o Pretensioner Double cab:
   Align the claws with the seat belt positioning holes and install the ELR of the seat belt with the bolt as shown in the illustration.

   Torque:
     4.8 N*m{ 49 kgf*cm , 42 in.*lbf }

1. w/ Pretensioner:
   Install the bolt and seat belt.

   Torque:
     4.8 N*m{ 49 kgf*cm , 42 in.*lbf } for bolt A

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf } for bolt B

1. w/ Pretensioner:
   Connect the pretensioner connector as shown in the illustration.

1. Single cab:
   Install the anchor with the bolt.

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf }

1. Close the cover.

1. Extra cab and double cab:
   Install the anchor with the bolt.

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf }

1. Install the cap.

1. Single cab:
   Install the quarter trim panel lower. Then install the seat belt floor anchor with the bolt.

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf }

1. Extra cab:
   Install the quarter inside trim board. Then install the seat belt floor anchor with the bolt.

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf }

1. Double cab:
   Install the anchor of the seat belt with the built-in bolt after installing the center pillar garnish lower.

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf }

22. INSTALL BACK PANEL GARNISH UPPER

1. Attach the 5 clips and 4 claws to install the garnish.

23. INSTALL FRONT PILLAR GARNISH LH

1. Attach the 2 clips and 2 claws to install the garnish.

1. w/ Assist grip:
   Install the assist grip with the 2 screws.

1. w/ Assist grip:
   Attach the 4 claws to install the 2 assist plugs.

24. INSTALL FRONT PILLAR GARNISH RH

HINT:

  Use the same procedures described for the LH side.

25. INSTALL COWL SIDE TRIM BOARD LH

1. Attach the 2 clips to install the trim board.

1. Install the cap nut.

26. INSTALL COWL SIDE TRIM BOARD RH

HINT:

  Use the same procedures described for the LH side.

27. INSTALL FRONT DOOR OPENING TRIM LH

28. INSTALL FRONT DOOR OPENING TRIM RH

29. INSTALL FRONT DOOR SCUFF PLATE LH

1. Attach the 4 clips and 8 claws to install the scuff plate.

30. INSTALL FRONT DOOR SCUFF PLATE RH

HINT:

  Use the same procedures described for the LH side.

31. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

32. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.