GSIC - Global Service Information Center

# FRONT SEAT ASSEMBLY (for Separate Seat Type) > REMOVAL

## for Preparation Click here

HINT:

1. Use the same procedures for the RH side and LH side.
2. The procedures listed below are for the LH side.

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE SEAT TRACK BRACKET COVER OUTER LH (Except Single Cab)

1. Using a screwdriver, detach the 2 claws.

   HINT:
     Tape the screwdriver tip before use.

1. Remove the bracket cover in the direction indicated by the arrow in the illustration.

3. REMOVE SEAT TRACK BRACKET COVER INNER LH (Except Single Cab)

1. Using a screwdriver, detach the 2 claws.

   HINT:
     Tape the screwdriver tip before use.

1. Remove the bracket cover in the direction indicated by the arrow in the illustration.

4. REMOVE FRONT SEAT HEADREST ASSEMBLY

5. REMOVE FRONT SEAT ASSEMBLY

1. Lift up the seat track adjusting handle and move the seat to the rearmost position.

1. Remove the 2 bolts on the front side of the seat.

1. Lift up the seat track adjusting handle and move the seat to the foremost position.

1. Remove the 2 bolts on the rear side of the seat.

1. Lift up the seat track adjusting handle and move the seat to the center position. Also, operate the reclining adjuster release handle and move the seatback to the upright position.

1. w/ Seat belt warning, w/ occupant detection sensor:
   Disconnect the connector under the seat.

1. Remove the seat.

   NOTICE:
     Be careful not to damage the vehicle body.