GSIC - Global Service Information Center

# TRANSMITTER BATTERY > INSTALLATION

1. INSTALL TRANSMITTER BATTERY

NOTICE:

  Take extra care when handling these precision electronic components.

1. Install a battery (lithium battery: CR2016) with the positive (+) side facing up, as shown in the illustration.

   NOTICE:
   1. Be sure that the positive (+) and negative (-) side of the transmitter battery are matched up correctly.
   2. Be careful not to bend the transmitter battery electrode during insertion.
   3. Keep the transmitter cover interior free of dust and oil.

1. Detach the hook of the transmitter battery's cover and install the cover.

2. INSTALL DOOR CONTROL TRANSMITTER MODULE

1. Install the door control transmitter module.

3. INSTALL TRANSMITTER HOUSING COVER

1. Install the transmitter housing cover to the transmitter housing case.

1. Check that the transmitter's LED illuminates 3 times when the switch is pressed 3 times.

   OK:
     Transmitter's LED illuminates 3 times when switch is pressed 3 times.