GSIC - Global Service Information Center

### FRONT DOOR BELT MOULDING > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE FRONT DOOR WINDOW REGULATOR HANDLE ASSEMBLY (w/o Power Window)

3. REMOVE FRONT DOOR LOWER FRAME BRACKET GARNISH LH

4. REMOVE DOOR PULL HANDLE

5. REMOVE FRONT ARMREST BASE PANEL UPPER LH (w/ Power Window)

6. REMOVE FRONT DOOR TRIM BOARD SUB-ASSEMBLY LH

7. REMOVE OUTER REAR VIEW MIRROR SUB-ASSEMBLY LH

8. REMOVE FRONT DOOR BELT MOULDING ASSEMBLY LH